|  |  |  |  |
| --- | --- | --- | --- |
| 300 watt projection lamp | | | |
| **lamp pictures** | | Luminous Flux  光通量 | 27000-30000LM |
| **Lighting Description** | |
|  | | Correlated Color Temperature./Wavel ength  相关色温 / 波长 | 8000K～8500K |
| CRI  显色指数 | 85Ra |
| Forward Voltage正向电压 | 12.5-18V |
| Operating Temperature  工作温度 | -40~60℃ |
| **光源** | | **灯具尺寸** | **transfer method** |
| **Lighting Resource** | | **lamp Size** | **change** |
| Light source type /  specification | High-power LED |  |  |
| Lamp beads | Sanan chip |
| Power supply model | MEAN WELL HLG-240-24A |
| product name | 300W LED outdoor rotating projection lamp |
| Product number | JWB300 |
| power | 300 watts |
| **灯具及电器** | |
| **Lamp and Electrical Equipment** | |
| Color temperature | 8000-8500K |

|  |  |  |
| --- | --- | --- |
| Light source life | ≥30,000 hours |  |
| Beam angle | 0.2 0.3（默认）  0.65 0.87 | Installation dimensions |
| Adjustable angle of | 0-180 ° |  |
| bracket |
| Projection distance | 6-100m |
| Rotation | Umbrella |
| transmission | tooth rotation |
| Lens size | 63MM high |
| temperature lamp |
| Imaging lens | 6-piece ultra-high- |
| definition |
| installation | ce mounted ceiling, s |
|  | Aviation cold forged |
| Cooling method | aluminum +  double row booster |
|  | fan |
| Protection level | IP65 outdoor |
| rainproof |
|  | Lightning |
| Security project | protection,  overcurrent and |
|  | overvoltage |
|  | Installation |
| mensions / opening s | dimensions  (see picture on the |
|  | right) |
| Lightning protection | IEC61000-4 (Level4) |
| ESD protection |
| Accessories | Pull out some screws |
| Weight of the | 7.5 kg |
| whole lamp |
| housing material and | Aluminum alloy |
| black |